(module SML1206 (layer F.Cu) (tedit 0)
  (descr "<b>SML10XXKH-TR (HIGH INTENSITY) LED</b><p>\n<table>\n<tr><td>SML10R3KH-TR</td><td>ULTRA RED</td></tr>\n<tr><td>SML10E3KH-TR</td><td>SUPER REDSUPER BLUE</td></tr>\n<tr><td>SML10O3KH-TR</td><td>SUPER ORANGE</td></tr>\n<tr><td>SML10PY3KH-TR</td><td>PURE YELLOW</td></tr>\n<tr><td>SML10OY3KH-TR</td><td>ULTRA YELLOW</td></tr>\n<tr><td>SML10AG3KH-TR</td><td>AQUA GREEN</td></tr>\n<tr><td>SML10BG3KH-TR</td><td>BLUE GREEN</td></tr>\n<tr><td>SML10PB1KH-TR</td><td>SUPER BLUE</td></tr>\n<tr><td>SML10CW1KH-TR</td><td>WHITE</td></tr>\n</table>\n\nSource: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF")
  (fp_text reference LED4 (at -2.095 -1.381 -180) (layer F.SilkS)
    (effects (font (size 1.2065 1.2065) (thickness 0.12065)) (justify left bottom))
  )
  (fp_text value "" (at 1.905 1.651 -180) (layer F.Fab)
    (effects (font (size 1.2065 1.2065) (thickness 0.12065)) (justify left bottom))
  )
  (fp_arc (start -1.5 0) (end -1.5 -0.5) (angle 180) (layer F.Fab) (width 0.2032))
  (fp_arc (start 1.5 0) (end 1.5 0.5) (angle 180) (layer F.Fab) (width 0.2032))
  (fp_line (start -1.55 -0.75) (end 1.55 -0.75) (layer F.Fab) (width 0.1016))
  (fp_line (start 1.55 0.75) (end -1.55 0.75) (layer F.Fab) (width 0.1016))
  (fp_circle (center -0.725 -0.525) (end -0.6625 -0.525) (layer F.SilkS) (width 0.125))
  (fp_poly (pts (xy -1.6 -0.4) (xy -1.15 -0.4) (xy -1.15 -0.8) (xy -1.6 -0.8)) (layer F.Fab) (width 0))
  (fp_poly (pts (xy -1.6 0.8) (xy -1.15 0.8) (xy -1.15 0.4) (xy -1.6 0.4)) (layer F.Fab) (width 0))
  (fp_poly (pts (xy -1.175 0.6) (xy -1 0.6) (xy -1 0.275) (xy -1.175 0.275)) (layer F.Fab) (width 0))
  (fp_poly (pts (xy 1.6 0.4) (xy 1.15 0.4) (xy 1.15 0.8) (xy 1.6 0.8)) (layer F.Fab) (width 0))
  (fp_poly (pts (xy 1.6 -0.8) (xy 1.15 -0.8) (xy 1.15 -0.4) (xy 1.6 -0.4)) (layer F.Fab) (width 0))
  (fp_poly (pts (xy 1.175 -0.6) (xy 1 -0.6) (xy 1 -0.275) (xy 1.175 -0.275)) (layer F.Fab) (width 0))
  (fp_poly (pts (xy -0.1 0.1) (xy 0.1 0.1) (xy 0.1 -0.1) (xy -0.1 -0.1)) (layer F.SilkS) (width 0))
  (pad C smd rect (at -1.75 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0635))
  (pad A smd rect (at 1.75 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
    (solder_mask_margin 0.0635))
)
