(footprint "4,1-PAD" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (descr "<b>MOUNTING PAD</b> 4.1 mm, round")
  (attr through_hole)
  (fp_text reference "H1" (at 0 0) (layer "F.SilkS") hide
    (effects (font (size 1.27 1.27) (thickness 0.15)))
    (tstamp 644ae9fc-3c8e-4089-866e-a12bf371c3e9)
  )
  (fp_text value "MOUNT-PAD-ROUND4.1" (at 0 0) (layer "F.SilkS") hide
    (effects (font (size 1.27 1.27) (thickness 0.15)))
    (tstamp 41acfe41-fac7-432a-a7a3-946566e2d504)
  )
  (fp_circle (center 0 0) (end 2.15 0) (layer "F.SilkS") (width 0.2032) (fill none) (tstamp 7f2301df-e4bc-479e-a681-cc59c9a2dbbb))
  (fp_circle (center 0 0) (end 4.572 0) (layer "F.SilkS") (width 0.1524) (fill none) (tstamp 98c78427-acd5-4f90-9ad6-9f61c4809aec))
  (fp_circle (center 0 0) (end 5.08 0) (layer "Dwgs.User") (width 2) (fill none) (tstamp 65134029-dbd2-409a-85a8-13c2a33ff019))
  (fp_arc (start 0 2.54) (mid -1.796051 1.796051) (end -2.54 0) (layer "F.Fab") (width 3.9116) (tstamp 3a52f112-cb97-43db-aaeb-20afe27664d7))
  (fp_arc (start 0 -2.54) (mid 1.796051 -1.796051) (end 2.54 0) (layer "F.Fab") (width 3.9116) (tstamp f4eb0267-179f-46c9-b516-9bfb06bac1ba))
  (fp_circle (center 0 0) (end 0.762 0) (layer "F.Fab") (width 0.4572) (fill none) (tstamp 8087f566-a94d-4bbc-985b-e49ee7762296))
  (pad "B4,1" thru_hole circle (at 0 0) (size 8 8) (drill 4.1) (layers *.Cu *.Mask)
    (solder_mask_margin 0.0635) (tstamp a8447faf-e0a0-4c4a-ae53-4d4b28669151))
)
